Par Statistics
Total Non-vccgnd Signals=37
Total Non-vccgnd Design Pins=45
Total Non-vccgnd Conns=45
Total Non-vccgnd Timing Constrained Conns=42
Phase 1 CPU=3.4 sec
Phase 2 CPU=3.5 sec
Phase 3 CPU=3.5 sec
Phase 4 CPU=4.1 sec
Phase 5 CPU=4.1 sec
Phase 6 CPU=4.1 sec
Phase 7 CPU=4.1 sec
Phase 8 CPU=4.1 sec
Phase 9 CPU=4.1 sec
Phase 10 CPU=4.1 sec
AvgWirelenPerPin Fanout 1=1.0
AvgWirelenPerPin Fanout 2=0.0
AvgWirelenPerPin Fanout 3=17.0
AvgWirelenPerPin Fanout 4=0.0
AvgWirelenPerPin Fanout 10=10.5
AvgWirelenPerPin Fanout 50=0.0
AvgWirelenPerPin Fanout 100=0.0
AvgWirelenPerPin Fanout 500=0.0
AvgWirelenPerPin Fanout 5000=0.0
AvgWirelenPerPin Fanout 20000=0.0
AvgWirelenPerPin Fanout 50000=0.0
AvgWirelenPerPin Fanout 100000=0.0
IRR Gamma=1.0000